**TECHNICAL DATA SHEET**

***A350 Grip***

***Anti-sliding for belts***

**Anti-sliding** product, which prevents transmission belts and conveyor belts from sliding on pulleys and drive rollers; extends the durability of power transmission equipment; increases driving power; reduces noise; maintains the original characteristics of rubber belts, rubber-coated fabric or fabric impregnated with elastomers; cleans; prevents tears and cracks; extends durability.  
**Available as spray**.

**APPLICATION AREAS:**mechanical workshops, different types of industrial use applications.

**USE:**   
Before applying the product, thoroughly clean the seat and the belt; it can be used indoors or outdoors; even if exposed to the elements, it resists water; it does not form any film layers; it does not attract dust and dirt.  
**Not recommended**: in environments with a significant presence of volatile solid materials (e.g. wadding and wool mills).

**FEATURES**

* Appearance: limpid liquid, straw-coloured
* Odour: characteristic
* Dropping point in °C, minimum value D-566: N.A.
* Flash point: below 0°C
* Relative density: about 0.90 gr/ml
* Water solubility: insoluble
* Lipid solubility: soluble
* Heavy metals: not present