**TECHNICAL DATA SHEET**

***A390 Leak Test***

***Leak detector***

Water-basedleak **detector**; it can be used for cold and hot, flammable, harmful gases, coolants, compressed air, on pipes, valves, glued, welded or threaded fittings, compressors, cooling and smoke circuits and conditioning systems.  
It does **not** corrode; it does **not** stain or damage plastics, rubber, steel, copper, light alloys, and so on. **Non**-flammable, **non**-toxic, **non**-corrosive and biodegradable.  
**Available as spray**.

**APPLICATION AREAS:**Mechanical industry in general, installations and hydraulics, different types of industrial use applications.

**USE:  
Apply** the product on the part that is to be checked; it locates gas leaks by producing bubbles.

**FEATURES**

* Appearance: white foamy
* Odour: none
* Dropping point in °C, minimum value D-566: N.A.
* Flash point: below 0°C
* Relative density: about 1.00 gr/ml
* Water solubility: soluble
* Lipid solubility: insoluble
* Heavy metals: not present