**TECHNICAL DATA SHEET**

***A385 Antispatter WB***

***Anti-adhesive for water-based welding***

Anti-spatter for water-based welding (H₂O) **avoids the adhesion** of slag and drops of welding to parts being processed and any other surface, without altering the quality of weld beads; **it does NOT contain silicone**; it protects from oxides and corrosion; **the following treatments are possible** for painting, galvanising and so on by simply cleaning; excess dirt and debris can be removed with a detergent.   
**Available as spray**.

**APPLICATION AREAS:**suitable for electrical and inert gas-based autogenous welds.

**USE:**apply the product on the relevant surfaces in the most appropriate way.

**FEATURES**

* Appearance: limpid liquid, straw-coloured.
* Odour: none
* Dropping point in °C, minimum value D-566: N.A.
* Flash point: below 0°C
* Relative density: about 1.00 gr/ml
* Water solubility: total
* Lipid solubility: insoluble
* Heavy metals: not present