**TECHNICAL DATA SHEET**

***Soluble lubri-coolant fluids***

***Performa***

***diethanolamine free***

**Main features**

**Performa mineral lubri-coolants are quality products with the following characteristics:**

- diethanolamine free

- specific for any production need

- prepared in respect of the environment and the user’s protection

- prepared without hexahydrotriazine bactericide, in compliance with the Ministerial Decree of 7 July 1999, which introduces the 24th Adaptation Directive EEC 98/73 - 67/548

**Performa mineral lubri-coolants diluted in water at the concentrations of use allow:**

- recycling in single or centralised machine tool tanks

- constant stability in hard water

- foam not to form with medium hard water

- a reduced chemical risk

- a reduced biological risk

**Field of application**

**Performa mineral lubri-coolants without diethanolamine are specific for:**

- significant removal on alloyed steels


- removals on malleable alloys

- removals on all metals

- removal and grinding on all metals

- grinding on steels

**Main characteristics of multi-purpose preparations**



**TECHNICAL DATA SHEET**

***Soluble lubri-coolant fluids***

***Performa***

***diethanolamine free***

**Application guide**

