**TECHNICAL DATA SHEET**

***G300 Unigrease***

***Multipurpose grease***

Multipurpose grease with excellent **adhesive** properties for works at high speed; **antioxidant**; it protects worked components from oxidation for a long time; **anticorrosive**;the strong penetration action ensures durable lubrication of the worked parts.

**Available as spray**.

**APPLICATION AREAS:**

mechanical workshops in general, automotive spare parts, for general maintenance, different types of industrial use applications; suitable to lubricate/grease bearings, power transmission equipment in general, articulated arms, metal chains, pivots, and so on.

**USE:**

apply the product in the most appropriate way.

**FEATURES**

* Appearance: straw-coloured, mushy
* Odour: characteristic
* Dropping point in °C, 450°C ASTM D-566: N.A.
* Flash point: below 0°C
* Relative density: about 0.85 gr/ml
* Water solubility: insoluble
* Lipid solubility: soluble
* Heavy metals: not present