**TECHNICAL DATA SHEET**

***F510 Tap Cut***

***Cutting oil for stainless steel***

Cutting oil suitable for any type of **STAINLESS** steel with a **lubricating** effect; it reduces friction with parts; improves cutting parameters; improves working finish; it is **cooling**; it improves the cutting edge of tools, increasing their durability; the product does not drip.  
**Available as spray and liquid.**

**APPLICATION AREAS:**mechanical workshops in general, for all drilling, turning and cutting operations of all types of **STAINLESS** steel.

**Spray USE:**apply the product on the parts to be worked or on the tool.

**Spray FEATURES**

* Appearance: brown liquid
* Odour: none
* Relative density: about 0.90 gr/ml
* Water solubility: insoluble
* Lipid solubility: soluble
* Heavy metals: not present

**Liquid USE:** apply the product without diluting, on the parts to be worked or on the tool, using a brush, atomiser, spraying systems or minimal lubrication systems.

**Liquid FEATURES**

* Appearance: brown liquid
* Relative density: about 0.90 gr/ml