**TECHNICAL DATA SHEET**

***A340 Stak***

***Silicone-based release agent without solvent***

Silicone-based **solvent-free** spray with high **anti-adhesive** and **sliding** properties; ideal as a release agent for moulds of plastic materials; **antioxidant** for the protection of mechanical parts in general; it **prevents material cracks**; a chemically neutral product.  
**Available as spray**.

**APPLICATION AREAS:**injection moulding or extrusion processes of plastic material and elastomers, such as sliding film for plastic/plastic or plastic/steel material couplings; protection and polishing of plastics and rubber.

**USE:**apply in the most appropriate way, according to the application description.  
**DO NOT SPRAY** close to paint lines and on anything that is to be subsequently painted or subject to surface treatment.

**FEATURES**

* Appearance: limpid liquid, colourless
* Odour: none
* pH: N.a.
* Flash point: below 0°C
* Relative density: about 0.90 gr/ml
* Water solubility: insoluble
* Lipid solubility: soluble
* Heavy metals: not present