**TECHNICAL DATA SHEET**

***G320 Vaselinegrease***

***Vaseline grease***

High quality **anti-adhesive** grease for joints and clamps; **anticorrosive**;it protects from corrosion of metals; **protective**;it prevents contact with air and water; anti-seizure; it reduces friction and avoids mechanical movements from locking; **it does not leave any residue, it does not harden and it does not stain.**

**Available as spray**.

**APPLICATION AREAS:**

mechanical workshops in general; food industry where there could be accidental contact with other substances; nautical; textile; different types of industrial use applications; to lubricate locks and hinges; for technical, domestic, DIY use, where there is a need of effective and clean lubrication.

**USE:**

apply the product in the most appropriate way.

**FEATURES:**

* Appearance: white liquid, mushy
* Odour: characteristic
* Flash point: below 0°C
* Relative density: about 0.85 gr/ml
* Water solubility: insoluble
* Lipid solubility: soluble
* Heavy metals: not present