**TECHNICAL DATA SHEET**

***L650 Chain Lub***

***Chain lubricant***

**Lubricant** for metal chains, stringy with high **adhesive power** and resistant to high pressures; the high **viscosity** guarantees the sliding of chains and bearings subject to high performance; it ensures durable lubrication and protects from **wear** and **oxidation**, **resistant to salt water** and **temperature swings**.  
During dispensing, the product penetrates the chain links, lubricating the internal rollers too. **It does NOT damage** rubber or plastic parts.   
**Available as spray**.

**APPLICATION AREAS:**for motion chains, gear and distribution chains, rims, pinions, open gears and mechanical moving parts.

**USE:**apply the product on the relevant surfaces in the most appropriate way.

**FEATURES**

* Appearance: limpid, straw-coloured liquid
* Odour: characteristic
* Flash point: below 0°C
* Relative density: about 0.90 gr/ml
* Water solubility: insoluble
* Lipid solubility: soluble
* Heavy metals: not present